IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "458817"
Time stamp: "2017-07-05T11:08:49"
Author: "BIM Author"
Author: "enquiries@pepgroup.co.uk"
Organization: "PEP Civil & Structures Ltd"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.5.0.0 - Alternate UI 16.5.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "PEP" "Modeller" (telecom address: e-mail "enquiries@pepgroup.co.uk") of Organization "PEP Civil & Structures Ltd" description "Civil & Structural Engineers"
  Owner history of Person "PEP" "Modeller" (telecom address: e-mail "enquiries@pepgroup.co.uk") of Organization "PEP Civil & Structures Ltd" description "Civil & Structural Engineers" | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1498056589 (2017-06-21T14:49:49Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "458817" | long name "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®" | phase "PRELIMINARY"
  IFCSITE "Default" | latitude 51° 44′ 29.89746″ | longitude -0° 31′ 47.131719″ | elevation above sea level 0.
    IFCBUILDING | postal address OFFICE: "PEP House", "Stoney Lane", "Hemel Hempstead,", "Hertfordshire", "HP1 2SB,", "UK" ("PEP House")
      IFCBUILDINGSTOREY "00 LEVEL DATUM" | long name "00 LEVEL DATUM" | elevation 0.
        contains 44 elements
          1 x IFCSLAB | object type "Floor:Pecavoid®CL-105" | names: "Floor:Pecavoid®CL-105:553314" | material: layers "Floor:Pecavoid®CL-105" ("MFL_PP TOP" 10., "MFL_Pecavoid" 105.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          21 x IFCBUILDINGELEMENTPROXY | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Graphics, Identity Data, Other
          1 x IFCSLAB | object type "Floor:Pecavoid®CS-150" | names: "Floor:Pecavoid®CS-150:590678" | material: layers "Floor:Pecavoid®CS-150" ("MFL_PP TOP" 2., "MFL_EPS 100" 50., "MFL_Pecavoid" 100.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CB-100" | names: "Floor:Pecavoid®CB-100:590937" | material: layers "Floor:Pecavoid®CB-100" ("MFL_PP TOP" 4.5, "MFL_Pecavoid" 100.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CB-175" | names: "Floor:Pecavoid®CB-175:665175" | material: layers "Floor:Pecavoid®CB-175" ("MFL_PP TOP" 4.5, "MFL_Pecavoid" 175.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CB-250" | names: "Floor:Pecavoid®CB-250:665202" | material: layers "Floor:Pecavoid®CB-250" ("MFL_PP TOP" 4.5, "MFL_Pecavoid" 250.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CB-300" | names: "Floor:Pecavoid®CB-300:665229" | material: layers "Floor:Pecavoid®CB-300" ("MFL_PP TOP" 4.5, "MFL_Pecavoid" 300.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CL-180" | names: "Floor:Pecavoid®CL-180:665467" | material: layers "Floor:Pecavoid®CL-180" ("MFL_PP TOP" 10., "MFL_Pecavoid" 180.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CL-255" | names: "Floor:Pecavoid®CL-255:665494" | material: layers "Floor:Pecavoid®CL-255" ("MFL_PP TOP" 10., "MFL_Pecavoid" 255.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CL-305" | names: "Floor:Pecavoid®CL-305:665521" | material: layers "Floor:Pecavoid®CL-305" ("MFL_PP TOP" 10., "MFL_Pecavoid" 305.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CS-225" | names: "Floor:Pecavoid®CS-225:665776" | material: layers "Floor:Pecavoid®CS-225" ("MFL_PP TOP" 2., "MFL_EPS 100" 50., "MFL_Pecavoid" 175.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CS-300" | names: "Floor:Pecavoid®CS-300:665803" | material: layers "Floor:Pecavoid®CS-300" ("MFL_PP TOP" 2., "MFL_EPS 100" 50., "MFL_Pecavoid" 250.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®CS-350" | names: "Floor:Pecavoid®CS-350:665830" | material: layers "Floor:Pecavoid®CS-350" ("MFL_PP TOP" 2., "MFL_EPS 100" 50., "MFL_Pecavoid" 300.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RDB-85" | names: "Floor:Pecavoid®RDB-85:666839" | material: layers "Floor:Pecavoid®RDB-85" ("MFL_PP TOP" 4.5, "MFL_Pecavoid" 85.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RDB-155" | names: "Floor:Pecavoid®RDB-155:666923" | material: layers "Floor:Pecavoid®RDB-155" ("MFL_PP TOP" 4.5, "MFL_Pecavoid" 155.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RDB-220" | names: "Floor:Pecavoid®RDB-220:666946" | material: layers "Floor:Pecavoid®RDB-220" ("MFL_PP TOP" 4.5, "MFL_Pecavoid" 220.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RDS-90" | names: "Floor:Pecavoid®RDS-90:668373" | material: layers "Floor:Pecavoid®RDS-90" ("MFL_PP TOP" 10., "MFL_Pecavoid" 90.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RDS-160" | names: "Floor:Pecavoid®RDS-160:668657" | material: layers "Floor:Pecavoid®RDS-160" ("MFL_PP TOP" 10., "MFL_Pecavoid" 160.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RDS-225" | names: "Floor:Pecavoid®RDS-225:668684" | material: layers "Floor:Pecavoid®RDS-225" ("MFL_PP TOP" 10., "MFL_Pecavoid" 225.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RD+-130" | names: "Floor:Pecavoid®RD+-130:668828" | material: layers "Floor:Pecavoid®RD+-130" ("MFL_PP TOP" 2., "MFL_EPS 100" 50., "MFL_Pecavoid" 130.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RD+-200" | names: "Floor:Pecavoid®RD+-200:669066" | material: layers "Floor:Pecavoid®RD+-200" ("MFL_PP TOP" 2., "MFL_EPS 100" 50., "MFL_Pecavoid" 200.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          1 x IFCSLAB | object type "Floor:Pecavoid®RD+-265" | names: "Floor:Pecavoid®RD+-265:669093" | material: layers "Floor:Pecavoid®RD+-265" ("MFL_PP TOP" 2., "MFL_EPS 100" 50., "MFL_Pecavoid" 265.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Pecavoid® Properties, BaseQuantities, Constraints, Dimensions
          2 x IFCBUILDINGELEMENTPROXY | object type "Model Text:1500mm Arial" | names: "Model Text:1500mm Arial" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Graphics, Identity Data, Other

Property sets
  Pset_SlabCommon | properties | on 21 objects (21 IFCSLAB)
    AcousticRating = "n/a" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "n/a" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "n/a" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "n/a" (IFCLABEL)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CL105" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CS 150" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CB 100" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CB 175" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CB 250" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CB 300" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CL180" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "Max Frank Ltd." (IFCLABEL)
    ModelReference = "Pecavoid® CL255" (IFCLABEL)
  Pset_ManufacturerTypeInformation: 13 more contents on 13 objects not shown
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 2.87999999999997 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 260mm 8/12 Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/55 Up to 1940mm 50/65" (IFCTEXT)
    CompressibleLegDepth = 105. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "Low Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CL" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "50" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "10-20" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 2.88000000000002 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 260mm 8/12 Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/55 Up to 1940mm 50/65" (IFCTEXT)
    CompressibleLegDepth = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "Low Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CS" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "50" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "10-20" (IFCTEXT)
    ThermalConductivity = "0.036 W/(m²K)" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    CompressibleLegDepth = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "Low Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "50" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "10-20" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    CompressibleLegDepth = 175. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "Medium Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "100" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "20-40" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    CompressibleLegDepth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "High Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "150" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "40-60" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    CompressibleLegDepth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "Very High Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "200" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "60+" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 2.87999999999997 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 260mm 8/12 Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/55 Up to 1940mm 50/65" (IFCTEXT)
    CompressibleLegDepth = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "Medium Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CL" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "100" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "20-40" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties | properties | on 1 object (1 IFCSLAB)
    Area = 2.87999999999997 (IFCAREAMEASURE) [SQUARE_METRE]
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 260mm 8/12 Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/55 Up to 1940mm 50/65" (IFCTEXT)
    CompressibleLegDepth = 255. (IFCLENGTHMEASURE) [MILLI METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    GroundShrinkagePotential = "High Shrinkage" (IFCTEXT)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Keynote = "E20/181" (IFCTEXT)
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CL" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    Phase Created = "New Construction" (IFCLABEL)
    Phase Demolished (no value)
    PredictedGroundMovement = "150" (IFCTEXT)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
    SoilPlasticityIndex = "40-60" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Pecavoid® Properties: 13 more contents on 13 objects not shown
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 2.87999999999997 [SQUARE_METRE]
    GrossVolume = 331.199999999997 [CUBIC_METRE]
    Perimeter = 7199.99999999995 [MILLI METRE]
    Width = 115. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 2.88000000000002 [SQUARE_METRE]
    GrossVolume = 437.760000000002 [CUBIC_METRE]
    Perimeter = 7200.00000000002 [MILLI METRE]
    Width = 152. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 0.720000000000005 [SQUARE_METRE]
    GrossVolume = 75.2400000000005 [CUBIC_METRE]
    Perimeter = 5400.00000000002 [MILLI METRE]
    Width = 104.5 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 0.720000000000005 [SQUARE_METRE]
    GrossVolume = 129.240000000001 [CUBIC_METRE]
    Perimeter = 5400.00000000002 [MILLI METRE]
    Width = 179.5 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 0.720000000000005 [SQUARE_METRE]
    GrossVolume = 183.240000000001 [CUBIC_METRE]
    Perimeter = 5400.00000000002 [MILLI METRE]
    Width = 254.5 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 0.720000000000005 [SQUARE_METRE]
    GrossVolume = 219.240000000002 [CUBIC_METRE]
    Perimeter = 5400.00000000002 [MILLI METRE]
    Width = 304.5 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 2.87999999999997 [SQUARE_METRE]
    GrossVolume = 547.199999999994 [CUBIC_METRE]
    Perimeter = 7199.99999999995 [MILLI METRE]
    Width = 190. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 2.87999999999997 [SQUARE_METRE]
    GrossVolume = 763.199999999992 [CUBIC_METRE]
    Perimeter = 7199.99999999995 [MILLI METRE]
    Width = 265. [MILLI METRE]
  BaseQuantities: 13 more contents on 13 objects not shown
  Constraints | properties | on 21 objects (21 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 00 LEVEL DATUM" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Level : 00 LEVEL DATUM" (IFCTEXT)
  Constraints | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Floor : Pecavoid®CS-150" (IFCTEXT)
  Constraints | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Work Plane = "<not associated>" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Floor : Pecavoid®CS-225" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Floor : Pecavoid®CS-300" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Floor : Pecavoid®CS-350" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Depth = 25. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 150. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 2.87999999999997 (IFCAREAMEASURE) [SQUARE_METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    Elevation at Bottom = -115. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Bottom Core = -115. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top Core = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 7199.99999999995 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 115. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.331199999999996 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 2.88000000000002 (IFCAREAMEASURE) [SQUARE_METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    Elevation at Bottom = -152. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Bottom Core = -152. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top Core = -2. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 7200.00000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 152. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.437760000000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    Elevation at Bottom = -104.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Bottom Core = -104.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top Core = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 5400.00000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 104.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0752400000000005 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    Elevation at Bottom = -179.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Bottom Core = -179.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top Core = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 5400.00000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 179.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.129240000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    Elevation at Bottom = -254.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Bottom Core = -254.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top Core = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 5400.00000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 254.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.183240000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 0.720000000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    ConcreteDepth = "In accordance with Structural Element" (IFCTEXT)
    Elevation at Bottom = -304.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Bottom Core = -304.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top Core = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 5400.00000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 304.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.219240000000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 16 more contents on 16 objects not shown
  Identity Data | properties | on 21 objects (21 IFCSLAB)
    SelectedGrade = "Refer to Pecavoid® Grades Table" (IFCTEXT)
  Identity Data | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Subcategory = "MFL_Pecavoid Text" (IFCLABEL)
  Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Subcategory = "Generic Models" (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "PEP Modeller" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Address = "PEP House, Stoney Lane, Bourne End, HP1 2SB" (IFCTEXT)
    Organization Contact No. = "01442869400" (IFCTEXT)
    Organization Description = "Civil & Structural Engineers" (IFCTEXT)
    Organization Name = "PEP Civil & Structures Ltd" (IFCTEXT)
    Revit Software Version = "Revit 2016 (or newer)" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "00 LEVEL DATUM" (IFCTEXT)
    Structural = TRUE (IFCBOOLEAN)
  Other | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Model Text: 600mm Arial" (IFCLABEL)
    Family and Type = "Model Text: 600mm Arial" (IFCLABEL)
    Type = "Model Text: 600mm Arial" (IFCLABEL)
    Type Id = "Model Text: 600mm Arial" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Model Text: 1500mm Arial" (IFCLABEL)
    Family and Type = "Model Text: 1500mm Arial" (IFCLABEL)
    Type = "Model Text: 1500mm Arial" (IFCLABEL)
    Type Id = "Model Text: 1500mm Arial" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Client" (IFCTEXT)
    PEP Project Number = "458817" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®" (IFCTEXT)
    Project Number = "458817" (IFCTEXT)
    Project Status = "PRELIMINARY" (IFCTEXT)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Pecavoid®CL-105" (IFCLABEL)
    Family and Type = "Floor: Pecavoid®CL-105" (IFCLABEL)
    Type = "Floor: Pecavoid®CL-105" (IFCLABEL)
    Type Id = "Floor: Pecavoid®CL-105" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Pecavoid®CS-150" (IFCLABEL)
    Family and Type = "Floor: Pecavoid®CS-150" (IFCLABEL)
    Type = "Floor: Pecavoid®CS-150" (IFCLABEL)
    Type Id = "Floor: Pecavoid®CS-150" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Pecavoid®CB-100" (IFCLABEL)
    Family and Type = "Floor: Pecavoid®CB-100" (IFCLABEL)
    Type = "Floor: Pecavoid®CB-100" (IFCLABEL)
    Type Id = "Floor: Pecavoid®CB-100" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Pecavoid®CB-175" (IFCLABEL)
    Family and Type = "Floor: Pecavoid®CB-175" (IFCLABEL)
    Type = "Floor: Pecavoid®CB-175" (IFCLABEL)
    Type Id = "Floor: Pecavoid®CB-175" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Pecavoid®CB-250" (IFCLABEL)
    Family and Type = "Floor: Pecavoid®CB-250" (IFCLABEL)
    Type = "Floor: Pecavoid®CB-250" (IFCLABEL)
    Type Id = "Floor: Pecavoid®CB-250" (IFCLABEL)
  Other: 17 more contents on 17 objects not shown
  Phasing | properties | on 44 objects (23 IFCBUILDINGELEMENTPROXY, 21 IFCSLAB)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 20 objects (20 IFCSLAB)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: n/a" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: n/a" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: n/a" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: n/a" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: n/a" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: n/a" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text:600mm Arial" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text:1500mm Arial" (IFCIDENTIFIER)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® CL105" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® CB 100" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® CS150" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® RDB 85" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® CB175" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® CB250" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® CB300" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Pecavoid® CL180" (IFCTEXT)
  Graphics: 15 more contents on 15 objects not shown
  General | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    NBSSpecificationPath = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Analytical Properties(Type) | properties | on 14 objects (14 IFCSLAB)
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Analytical Properties(Type) | properties | on 7 objects (7 IFCSLAB)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.72 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.38888888888889 (IFCREAL)
    Thermal mass = 2598.77 (IFCREAL)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 115. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 152. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 104.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 179.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 254.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 304.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 190. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 265. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Exterior" (IFCIDENTIFIER)
  Construction(Type): 13 more contents on 13 objects not shown
  Data(Type) | properties | on 7 objects (7 IFCSLAB)
    Applications = "For use beneath reinforced concrete floor slabs and pilecaps." (IFCTEXT)
    GradeOptions = "Refer to AvailableGrade perameter under Identity Data" (IFCTEXT)
    InsulationThermalResistance = "n/a" (IFCTEXT)
    InsulationThickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThirdPartyCertification = "BA 12/4923" (IFCTEXT)
    WidthOptions = "n/a" (IFCTEXT)
  Data(Type) | properties | on 7 objects (7 IFCSLAB)
    Applications = "For use beneath reinforced concrete floor slabs." (IFCTEXT)
    GradeOptions = "Refer to AvailableGrade perameter under Identity Data" (IFCTEXT)
    InsulationThermalResistance = "1.39(m²·K)/W" (IFCTEXT)
    InsulationThickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThirdPartyCertification = "BA 12/4923" (IFCTEXT)
    WidthOptions = "n/a" (IFCTEXT)
  Data(Type) | properties | on 7 objects (7 IFCSLAB)
    Applications = "For use beneath reinforced concrete ground beams." (IFCTEXT)
    GradeOptions = "Refer to AvailableGrade perameter under Identity Data" (IFCTEXT)
    InsulationThermalResistance = "n/a" (IFCTEXT)
    InsulationThickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThirdPartyCertification = "BA 12/4923" (IFCTEXT)
    WidthOptions = "Manufactured width 25mm incraments for widths between 300mm and 800mm ; Manufactured width 50mm incraments for widths between 800mm and 1200mm" (IFCTEXT)
  Dimensions(Type) | properties | on 2 objects (2 IFCSLAB)
    CompressibleLegDepth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 2 objects (2 IFCSLAB)
    CompressibleLegDepth = 225. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 1 object (1 IFCSLAB)
    CompressibleLegDepth = 105. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 1 object (1 IFCSLAB)
    CompressibleLegDepth = 150. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 1 object (1 IFCSLAB)
    CompressibleLegDepth = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 1 object (1 IFCSLAB)
    CompressibleLegDepth = 175. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 1 object (1 IFCSLAB)
    CompressibleLegDepth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 1 object (1 IFCSLAB)
    CompressibleLegDepth = 180. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type): 11 more contents on 11 objects not shown
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CL-105" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CS-150" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CB-100" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CB-175" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CB-250" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CB-300" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CL-180" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type) | properties | on 1 object (1 IFCSLAB)
    Author = "PEP Civil and Structures Ltd" (IFCTEXT)
    BIMObjectName = "MaxFrankLtd_CompressibleBoardSubstructureFormwork_Pecavoid®CL-255" (IFCTEXT)
    ManufacturerName = "Max Frank Ltd" (IFCTEXT)
    ManufacturerURL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Title = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Version = "Products v1.5" (IFCTEXT)
    Version = "1.1" (IFCTEXT)
  General(Type): 13 more contents on 13 objects not shown
  Graphics(Type) | properties | on 21 objects (21 IFCSLAB)
    Coarse Scale Fill Color = 5577216 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Crosshatch 1. 6" (IFCLABEL)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "600mm Arial" (IFCTEXT)
  Identity Data(Type) | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "1500mm Arial" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 260mm 8/12 Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/55 Up to 1940mm 50/65" (IFCTEXT)
    Description = "Heave Precaution to underside of foundation" (IFCTEXT)
    GroundShrinkagePotential = "Low Shrinkage" (IFCTEXT)
    Keynote = "E20/181" (IFCTEXT)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CL" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    PredictedGroundMovement = "50" (IFCTEXT)
    SoilPlasticityIndex = "10-20" (IFCTEXT)
    Type Comments = "High Shrinkability Potential" (IFCTEXT)
    Type Name = "Pecavoid®CL-105" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 260mm 8/12 Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/55 Up to 1940mm 50/65" (IFCTEXT)
    Description = "Heave Precaution to underside of foundation" (IFCTEXT)
    GroundShrinkagePotential = "Low Shrinkage" (IFCTEXT)
    Keynote = "E20/181" (IFCTEXT)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CS" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    PredictedGroundMovement = "50" (IFCTEXT)
    SoilPlasticityIndex = "10-20" (IFCTEXT)
    ThermalConductivity = "0.036 W/(m²K)" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "Pecavoid®CS-150" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    Description = "Heave Precaution to underside of foundation" (IFCTEXT)
    GroundShrinkagePotential = "Low Shrinkage" (IFCTEXT)
    Keynote = "E20/181" (IFCTEXT)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    PredictedGroundMovement = "50" (IFCTEXT)
    SoilPlasticityIndex = "10-20" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "Pecavoid®CB-100" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    Description = "Heave Precaution to underside of foundation" (IFCTEXT)
    GroundShrinkagePotential = "Medium Shrinkage" (IFCTEXT)
    Keynote = "E20/181" (IFCTEXT)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    PredictedGroundMovement = "100" (IFCTEXT)
    SoilPlasticityIndex = "20-40" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "Pecavoid®CB-175" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    Description = "Heave Precaution to underside of foundation" (IFCTEXT)
    GroundShrinkagePotential = "High Shrinkage" (IFCTEXT)
    Keynote = "E20/181" (IFCTEXT)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    PredictedGroundMovement = "150" (IFCTEXT)
    SoilPlasticityIndex = "40-60" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "Pecavoid®CB-250" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    AvailableGrade = "CONCRETE DEPTH GRADE Up to 340mm 10/15 Up to 540mm 15/22 Up to 740mm 20/30 Up to 940mm 25/35 Up to 1140mm 30/40 Up to 1340mm 35/45 Up to 1540mm 40/50 Up to 1740mm 45/60 Up to 1940mm 50/70" (IFCTEXT)
    Description = "Heave Precaution to underside of foundation" (IFCTEXT)
    GroundShrinkagePotential = "Very High Shrinkage" (IFCTEXT)
    Keynote = "E20/181" (IFCTEXT)
    Manufacturer = "Max Frank Ltd." (IFCTEXT)
    Model = "Pecavoid® CB" (IFCTEXT)
    NRM1 = "1.1.2 / 1.1.3" (IFCTEXT)
    PredictedGroundMovement = "200" (IFCTEXT)
    SoilPlasticityIndex = "60+" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "Pecavoid®CB-300" (IFCTEXT)
    URL = "http://www.maxfrank.co.uk/uk/products/formwork-technologies/pecavoid-cellular-void-former.php" (IFCTEXT)
    Uniclass1.4 = "L31 / L332" (IFCTEXT)
    Uniclass2015 = "Ss_20_80_60" (IFCTEXT)
  Identity Data(Type): 16 more contents on 16 objects not shown
  Other(Type) | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Model Text" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_16:Compressible board substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "Floor" (IFCTEXT)
    Features = "Easy to install,needs no ancillaries and requires minimal excavation. Can be incorporated with Pecafil® permanent formwork system. Does not degrade and contains no CFCs or HCFCs. Reduction in loads transmitted to structure. Cost effective and available in a range of grades and types. Suitable for most suspended slabs and beams. Offers improved insulation and enhanced sustainability. Can be supplied with drainage channels for high water tables." (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene closed cell with 10mm heavy duty polypropylene top by Max Frank Ltd." (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Pecavoid® CL105" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_Pecavoid®CL-105" (IFCTEXT)
    NominalHeight = 115. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 115" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Floors" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "Floor" (IFCTEXT)
    Features = "Easy to install,needs no ancillaries and requires minimal excavation. Can be incorporated with Pecafil® permanent formwork system. Does not degrade and contains no CFCs or HCFCs. Reduction in loads transmitted to structure. Cost effective and available in a range of grades and types. Suitable for most suspended slabs and beams. Offers improved insulation and enhanced sustainability. Can be supplied with drainage channels for high water tables." (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene closed cell with 50mm EPS panel and with 2mm heavy duty polypropylene top by Max Frank Ltd." (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Pecavoid® CS 150" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_Pecavoid®CS-150" (IFCTEXT)
    NominalHeight = 152. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 152" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_16:Compressible board substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "Floor" (IFCTEXT)
    Features = "Easy to install,needs no ancillaries and requires minimal excavation. Can be incorporated with Pecafil® permanent formwork system. Does not degrade and contains no CFCs or HCFCs. Reduction in loads transmitted to structure. Cost effective and available in a range of grades and types. Suitable for most suspended ground beams. Offers improved insulation and enhanced sustainability. Can be supplied with drainage channels for high water tables." (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene closed cell with 4.5mm heavy duty polypropylene top by Max Frank Ltd." (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Pecavoid® CB 100" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_Pecavoid®CB-100" (IFCTEXT)
    NominalHeight = 104.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x (300) x 104.5" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_16:Compressible board substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "Floor" (IFCTEXT)
    Features = "Easy to install,needs no ancillaries and requires minimal excavation. Can be incorporated with Pecafil® permanent formwork system. Does not degrade and contains no CFCs or HCFCs. Reduction in loads transmitted to structure. Cost effective and available in a range of grades and types. Suitable for most suspended ground beams. Offers improved insulation and enhanced sustainability. Can be supplied with drainage channels for high water tables." (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene closed cell with 4.5mm heavy duty polypropylene top by Max Frank Ltd." (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Pecavoid® CB 175" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_Pecavoid®CB-175" (IFCTEXT)
    NominalHeight = 179.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x (300) x 179.5" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Floors" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "Floor" (IFCTEXT)
    Features = "Easy to install,needs no ancillaries and requires minimal excavation. Can be incorporated with Pecafil® permanent formwork system. Does not degrade and contains no CFCs or HCFCs. Reduction in loads transmitted to structure. Cost effective and available in a range of grades and types. Suitable for most suspended ground beams. Offers improved insulation and enhanced sustainability. Can be supplied with drainage channels for high water tables." (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene closed cell with 4.5mm heavy duty polypropylene top by Max Frank Ltd." (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Pecavoid® CB 250" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_Pecavoid®CB-250" (IFCTEXT)
    NominalHeight = 254.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x (300) x 254.5" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Floors" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "Floor" (IFCTEXT)
    Features = "Easy to install,needs no ancillaries and requires minimal excavation. Can be incorporated with Pecafil® permanent formwork system. Does not degrade and contains no CFCs or HCFCs. Reduction in loads transmitted to structure. Cost effective and available in a range of grades and types. Suitable for most suspended ground beams. Offers improved insulation and enhanced sustainability. Can be supplied with drainage channels for high water tables." (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene closed cell with 4.5mm heavy duty polypropylene top by Max Frank Ltd." (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Pecavoid® CB 300" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_Pecavoid®CB-300" (IFCTEXT)
    NominalHeight = 304.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x (300) x 304.5" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Floors" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "Floor" (IFCTEXT)
    Features = "Easy to install,needs no ancillaries and requires minimal excavation. Can be incorporated with Pecafil® permanent formwork system. Does not degrade and contains no CFCs or HCFCs. Reduction in loads transmitted to structure. Cost effective and available in a range of grades and types. Suitable for most suspended slabs and beams. Offers improved insulation and enhanced sustainability. Can be supplied with drainage channels for high water tables." (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene closed cell with 10mm heavy duty polypropylene top by Max Frank Ltd." (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Pecavoid® CL180" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_Pecavoid®CL-180" (IFCTEXT)
    NominalHeight = 190. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 190" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Other(Type): 15 more contents on 15 objects not shown
  Text(Type) | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Text(Type) | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  Materials and Finishes(Type) | properties | on 1 object (1 IFCSLAB)
    Structural Material = "MFL_Pecavoid" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)